**Assignment Submission**

**Heading: Introduction to Exec-Timeout**

**Approach:** Analysed both the switches. Both the switches were connected to vlan1 and having up/up status. For senior switch secret password is hack. Mainly, need to change the configuration on both switches. Senior: Going in global Configuration mode using ‘line con 0’ then ‘exec-timeout’ command, this command will disconnect the session after the time period of inactivity. Similarly, enable ‘exec-timeout’ in admin.

**Solution:** Enabled exec-timeout command in both the switches.